Hextronik HXT900 - 9g Micro Servo
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Basic Information
	Modulation: 
	Analog 

	Torque: 
	4.8V:
22.2 oz-in (1.60 kg-cm)

	Speed: 
	4.8V:
0.12 sec/60°

	Weight: 
	0.32 oz (9.1 g) 

	Dimensions: 
	Length:
0.83 in (21.0 mm)
Width:
0.47 in (12.0 mm)
Height:
0.87 in (22.0 mm) 

	Motor Type: 
	Coreless 

	Gear Type: 
	Plastic 

	Rotation/Support: 
	Bushing 


Additional Specifications
	Rotational Range: 
	90° 

	Pulse Cycle: 
	20 ms 

	Pulse Width: 
	450-2450 µs 

	Connector Type: 
	JR 



image1.jpeg




image2.gif




